{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":76,"n_cols":7,"rows_kept":76,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHHE-CV37"]
[]
[]
[]
[]
["","","","","","EKHHE200CV37","EKHHE260CV37"]
["Opwarmtijd","Max.","","","uu:mm","06:27:00","09:29:00"]
["COP","","","","","3.23","3.37"]
["Sanitair warm water","Rendement","","Nom","kW","1.339","1249"]
["Equivalent warm water","Max.","","","l","247","340"]
["Afmetingen","Unit","","Hoogte","mm","1607","1892"]
["","","","Diameter","mm","621","621"]
["Gewicht","Unit","","Leeg","kg","85","97"]
["","","","Vol","kg","277","347"]
["Afmetingen","Unit","H","Geïntegreerd in binnendeel","mm","1607","1892"]
["Gewicht","Verpakte unit","","","kg","96","109"]
["Montageplaats","","","","","Binnen","Binnen"]
["IP-klasse","","","","","IP24","IP24"]
["Compressor","Type","","","","Roterend","Roterend"]
["Koelmiddel","Type","","","","R-134a","R-134a"]
["Warmtepomp","Naam","","","","EKHHE200CV37","EKHHE260CV37"]
["Koelmiddel","GWP","","","","1430","1430"]
["Koudemiddel","Vulling","","","tCO2Eq","1.43","1.43"]
["Koelmiddel","Vulling","","","kg","1","1"]
["Warmtepomp","Totale verwarmingscapaciteit","","","kW","0.43","0.43"]
["","Omkasting","","Kleur","","Wit","Wit"]
["","Afmetingen","Unit","H","mm","1607","1892"]
["","","","B","mm","621","621"]
["","","","D","mm","621","621"]
["","Gewicht","","Unit","kg","85","97"]
["","","","Verpakte unit","kg","96","109"]
["","Montageplaats","","","","Enkel binnen","Enkel binnen"]
["","Montage","","IP-klasse","","IP24","IP24"]
["","","","Afstand van de muur","mm","200","200"]
["","Werkingsbereik","Omgeving","Min.","°CDB","-7","-7"]
["","","","Max.","°CDB","43","43"]
["","Geluidsdrukniveau op 1m","","Nom.","dB(A)","53","51"]
["","","","Fluisterstille nachtstand","dB(A)","53.0","51"]
["","Koudemiddel","","Type","","R-134A","R-134A"]
["","","","GWP","","1430","1430"]
["","","","Vulling","tCO2Eq","1.43","1.43"]
["","","","Inhoud","kg","1","1"]
["","Ontdooimethode","","","","Heet gas-ontdooiing","Heet gas-ontdooiing"]
["","Systeemdruk","","Max.","bar","7","7"]
["Tank","Vermogen ingebouwd verwarmingselement ","","Nom.","kW","1.5","1.5"]
["","Omkasting","","Kleur","","Wit","Wit"]
["","","","Materiaal","","Geëmailleerd staal","Geëmailleerd staal"]
["","Montageplaats","","","","Enkel binnen","Enkel binnen"]
["","Montage","","IP-klasse","","IP24","IP24"]
["","","","Aansluiting op zonne-installatie mogelijk","","Nee","Nee"]
["","","","Recirculatie-opening tank","","Nee","Nee"]
["Algemeen","Productbeschrijving","","Lucht/water-warmtepomp","","Ja","Ja"]
["","","","Identificatie model","","EKHHE200CV37","EKHHE260CV37"]
["","Extra verwarmingselement","","Type stroomvoorziening","","Elektriciteit","Elektriciteit"]
["","Gegevens van leverancier/fabrikant","","Naam of handelsmerk","","Daikin Europe N.V.","Daikin Europe N.V."]
["","LW(A) geluidsvermogensniveau (volgens EN14825)","","Binnen","dB(A)","53","51"]
["Verwarming van sanitair warm water","Algemeen","","Aangegevens belastingprofiel","","L","XL"]
["","","","Functie voor verwarmen van water tijdens daluren","","Ja","Ja"]
["","","","Energierendementsklasse waterverwarming","","A+","A+"]
["Sanitair warm water","Algemeen","","Ingest. temp. thermostaat","°C","55","55"]
["Geluidsniveau","Sanitair warm water","","Buitenunit","dB(A)","45","44"]
["","","","Binnenunit","dB(A)","53","51"]
["Verwarming van sanitair warm water","Gematigd klimaat","","AEC (jaarlijks stroomverbruik)","kWh","761","1210"]
["","","","Qelec (dagelijks stroomverbruik)","kWh","2.08","3.31"]
["","Koud klimaat","","AEC (jaarlijks stroomverbruik)","kWh","944","1496"]
["","","","Qelec (dagelijks stroomverbruik)","kWh","2.59","4.10"]
["","Warm klimaat","","AEC (jaarlijks stroomverbruik)","kWh","631","1046"]
["","","","Qelec (dagelijks stroomverbruik)","kWh","1.73","2.87"]
["Warmtepomp","Spanningsvorm","","Fase","","1P","1P"]
["","","","Frequentie","Hz","50","50"]
["","","","Spanning","V","230","230"]
["","","","Max. bedrijfsstroom","A","8.5","8.5"]
["","","","Aanbevolen plaatselijk gebruik","A","2.43","2.43"]
["Tank","Spanningsvorm","","Fase","","1P","1P"]
["","","","Frequentie","Hz","50","50"]
["","","","Spanning","V","230","230"]