{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":7,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHTS-AC"]
[]
[]
[]
[]
["","","","","","EKHTS200AC","EKHTS260AC"]
["Afmetingen","Unit","","Breedte","mm","600","600"]
["","","Hoogte","Tank","mm","1,335","1,610"]
["","","","Geïntegreerd in binnendeel","mm","2,010","2,285"]
["","","","Diepte","mm","695","695"]
["Behuizing","Materiaal","","","","Gegalvaniseerd staal (voorgelakte metaalplaat)","Gegalvaniseerd staal (voorgelakte metaalplaat)"]
["","Colour","","","","Metaalgrijs","Metaalgrijs"]
["Tank","Energie-efficiëntieklasse","","","","B","B"]
["","Materiaal","","","","Roestvrij staal (EN 1.4521)","Roestvrij staal (EN 1.4521)"]
["","Permanent warmteverlies","","","W","50","63"]
["","Watervolume","","","l","200","260"]
["Gewicht","Unit","","Leeg","kg","70","78"]