{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":8,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWP-B"]
[]
[]
[]
[]
["","","","","","EKHWP300B","EKHWP54419BA","EKHWP500B"]
["Warmtewisselaar","Warmtapwater","","Leidingmateriaal","","","Roestvrij staal (DIN 1.4404)"]
["","","","Bedrijfsdruk","bar","","10.0"]
["","","","Volume interne spiraal","l","","28.9"]
["","","","Hoeveelheid","","","1"]
["","Vullen","","Hoeveelheid","","","1"]
["","","","Leidingmateriaal","","","Roestvrij staal (DIN 1.4404)"]
["","","","Bedrijfsdruk","bar","","3.0"]
["","","","Volume interne spiraal","l","","10.0"]
["","Hulpzonneverwarming","","Volume interne spiraal","l","","3.9"]
["","","","Leidingmateriaal","","","Roestvrij staal (DIN 1.4404)"]
["","","","Bedrijfsdruk","bar","","3.0"]
["","","","Hoeveelheid","","","1"]
["Afmetingen","Unit","","Breedte","mm","","790"]
["","","Hoogte","Tank","mm","","1,658"]
["","","","Diepte","mm","","790"]
["Casing","Material","","","","","Slagvast polypropyleen"]
["","Colour","","","","","Verkeerswit (RAL9016)/Donkergrijs (RAL7011)"]
["Tank","Energie-efficiëntieklasse","","","","","B"]
["","Maximumwatertemperatuur","","","°C","","85"]
["","Materiaal","","","","","Polypropyleen"]
["","Watervolume","","","l","","477"]
["Gewicht","Unit","","Leeg","kg","","71"]
["","","","Vol","kg","","548"]
["Montage (2)","","","","","","Vloer"]
["Opmerkingen","","","","","(1) - Heatloss according to EN12897","(1) - Warmteverlies volgens EN12897","(1) - Heatloss according to EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","","(5) - For tapping volume 140l -> 5820 Wh (bath) / 8kW heat pump","(5) - Voor een aftapvolume van 140l -> 5820 Wh (bad) / 8kW warmtepomp","(5) - For tapping volume 140l -> 5820 Wh (bath) / 16kW heat pump"]
["","","","","","(6) - For tapping volume 90l -> 3660 Wh (bath) / 8kW heat pump","(6) - Voor een aftapvolume van 90l -> 3660 Wh (bad) / 8kW warmtepomp","(6) - For tapping volume 90l -> 3660 Wh (bath) / 16kW heat pump"]
["","","","","","","(7) - Voor een aftapvolume van 140l -> 5820 Wh (bad) / 16kW warmtepomp"]
["","","","","","","(8) - Voor een aftapvolume van 90l -> 3660 Wh (bad) / 16kW warmtepomp"]
["","","","","","","(9) - Warmtewisselaar parallel aangesloten, TKW= 10°C/ TWW= 45°C/ TSP= 65°C/ Pload= 35kW/ Tflow= 80°C"]
["","","","","","","(10) - TKW= 10°C/ TWW= 45°C/ TSP= 65°C/ Pload= 35kW/ Tflow= 80°C"]
["Montage (2)","","","","","Vloer","","Vloer"]
["Behuizing","Kleur","","","","Verkeerswit (RAL9016)/Donkergrijs (RAL7011)","","Verkeerswit (RAL9016)/Donkergrijs (RAL7011)"]
["","Materiaal","","","","Slagvast polypropyleen","","Slagvast polypropyleen"]
["Afmetingen","Unit","H","Tank","mm","1646","","1658"]
["","","","Breedte","mm","595","","790"]
["","","","Diepte","mm","615","","790"]
["Gewicht","Unit","","Leeg","kg","53","","76"]
["","","","Vol","kg","347","","553"]
["Tank","Watervolume","","","l","294","","477"]
["","Materiaal","","","","Polypropyleen","","Polypropyleen"]
["","Maximumwatertemperatuur","","","°C","85","","85"]
["","Energie-efficiëntieklasse","","","","B","","B"]
["Warmtewisselaar","Warmtapwater","","Hoeveelheid","","1","","1"]
["","","","Leidingmateriaal","","Roestvrij staal (DIN 1.4404)","","Roestvrij staal (DIN 1.4404)"]
["","","","Volume interne spiraal","l","27.8","","28.9"]
["","","","Bedrijfsdruk","bar","10.0","","10.0"]
["","Vullen","","Hoeveelheid","","1","","1"]
["","","","Leidingmateriaal","","Roestvrij staal (DIN 1.4404)","","Roestvrij staal (DIN 1.4404)"]
["","","","Volume interne spiraal","l","12.9","","18.1"]
["","","","Bedrijfsdruk","bar","6.0","","6.0"]
["","Hulpzonneverwarming","","Hoeveelheid","","","","1"]
["","","","Leidingmateriaal","","","","Roestvrij staal (DIN 1.4404)"]
["","","","Volume interne spiraal","l","","","3.9"]
["","","","Bedrijfsdruk","bar","","","3.0"]