{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWSP-D3V3"]
[]
[]
[]
[]
["","","","","","EKHWSP150D3V3","EKHWSP180D3V3","EKHWSP200D3V3","EKHWSP250D3V3","EKHWSP300D3V3"]
["Omkasting","Kleur","","","","Neutraal wit","Neutraal wit","Neutraal wit","Neutraal wit","Neutraal wit"]
["","Materiaal","","","","Met epoxy gecoat staal, Met epoxy gecoat zacht staal","Met epoxy gecoat staal, Met epoxy gecoat zacht staal","Met epoxy gecoat staal, Met epoxy gecoat zacht staal","Met epoxy gecoat staal, Met epoxy gecoat zacht staal","Met epoxy gecoat staal, Met epoxy gecoat zacht staal"]
["Afmetingen","Unit","Hoogte","Tank","mm","1,000","1,164","1,264","1,535","1,745"]
["","","","Diameter","mm","595","595","595","595","595"]
["Gewicht","Unit","","Leeg","kg","45","50","53","58","63"]
["","","","Vol","kg","190","224","245","300","355"]
["Tank","Watervolume","","","l","145","174","192","242","292"]
["","Materiaal","","","","Roestvrij staal (EN 1.4521)","Roestvrij staal (EN 1.4521)","Roestvrij staal (EN 1.4521)","Roestvrij staal (EN 1.4521)","Roestvrij staal (EN 1.4521)"]
["","Maximumwatertemperatuur","","","°C","75","75","75","75","75"]
["","Energie-efficiëntieklasse","","","","B","B","B","B","B"]
["Warmtewisselaar","Warmtapwater","","Hoeveelheid","","1","1","1","1","1"]
["","","","Leidingmateriaal","","Stainless steel (EN 1.4521)","Stainless steel (EN 1.4521)","Stainless steel (EN 1.4521)","Stainless steel (EN 1.4521)","Stainless steel (EN 1.4521)"]
["","","","Volume interne spiraal","l","4.9","6.5","8.2","8.2","8.2"]
["","","","Bedrijfsdruk","bar","10","10","10","10","10"]
["Boosterverwarmer","Capaciteit","","","kW","3","3","3","3","3"]
["Opmerkingen","","","","","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897"]