{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELBH-E9W"]
[]
[]
[]
[]
["","","","","","ELBH12EF9W (Archived)"]
["Behuizing","Kleur","","","","Wilt + zwart"]
["","Materiaal","","","","Kunsthars, metaalplaat"]
["Afmetingen","Unit","","Hoogte","mm","840"]
["","","","Breedte","mm","440"]
["","","","Diepte","mm","390"]
["Gewicht","Unit","","","kg","48.5"]
["PED (richtlijn drukapparatuur)","Categorie","","","","Categorie II"]
["Geluidsvermogenniveau","Nom.","","","dB(A)","44.0 (3)"]
["Geluidsdrukniveau op 1 m","Nom.","","","dB(A)","30.0 (4)"]
["Werkingsbereik","Verwarmen","waterzijdig","Min.","°C","15 (5)"]
["","","","Max.","°C","65 (5)"]
["","Koelen","","Min.","°CDB","10 (5)"]
["","","Waterzijde","Min.","°C","5 (5)"]
["","","","Max.","°C","22 (5)"]
["Voeding","Naam","","","","Zie opmerking 6"]
["Elektrische verwarming","Spanningsvorm","","Naam","","9W"]
["","","","Fase","","3~"]
["","","","Frequentie","Hz","50"]
["","","","Spanning","V","400"]
["","Afzekerwaarde","","","A","20.000 (7)"]
["Opmerkingen","","","","","(1) - Het bedrijfsbereik is uitgebreid tot lagere debieten, afhankelijk van de bedrijfsmodus - raadpleeg de ESP-curve."]
["","","","","","(2) - Exclusief het watervolume in de unit. Dit voulme garandeert dat er voldoende energie is voor het ontdooien van alle applicaties. Het volume moet echter worden vermenigvuldigd met 0,66 als de ingestelde temperatuur van de verwarming ≥ 45°C is (bv. bij ventilatorconvectors)."]
["","","","","","(3) - Gemeten bij een drukdaling van 10 kPa in het verwarmingssysteem met een uitgaande watertemperatuur van 47-55°C in een kamer met een omgevingstemperatuur van 20°C DB/WB 7°C/6°."]
["","","","","","(4) - De geluidswaarden worden in een semi-echoloze ruimte gemeten. Het geluidsdrukniveau is een relatieve waarde, die afhankelijk is van de afstand en de akoestische omgeving. Zie de geluidsniveautekeningen voor meer bijzonderheden. Het geluidsvermogenniveau is een absolute waarde die"]
["","","","","","(5) - Raadpleeg de werkbereik-tekening voor meer informatie"]
["","","","","","(6) - 4-polige zekering 20 A curve 400 V klasse C (zie bedradingsschema)"]