{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERRQ-AY1"]
[]
[]
[]
[]
["","","","","","ERRQ011AAY1","ERRQ014AAY1","ERRQ016AAY1"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Nom.","dB(A)","52","53","55"]
["Standaard-accessoires","Montagehandleiding","","","","1","1","1"]
["Geluidsvermogenniveau","Verwarmen","","Nom.","dB(A)","68","69","71"]
["Koelmiddel","Charge","","","TCO2Eq","9.4","9.4","9.4"]
["","GWP","","","","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","4.5","4.5","4.5"]
["","Type","","","","R-410A","R-410A","R-410A"]
["Afmetingen","Unit","","Breedte","mm","900","900","900"]
["","","","Diepte","mm","320","320","320"]
["","","","Hoogte","mm","1,345","1,345","1,345"]
["Werkingsbereik","Verwarmen","","Max.","°CWB","20","20","20"]
["","","","Min.","°CWB","-20","-20","-20"]
["","Warmtapwater","","Min.","°CDB","-20","-20","-20"]
["","","","Max.","°CDB","35","35","35"]
["Gewicht","Unit","","","kg","120","120","120"]
["Leidingaansluitingen","Thermische isolatie","","","","Zowel vloeistof- als gasleidingen","Zowel vloeistof- als gasleidingen","Zowel vloeistof- als gasleidingen"]
["","Vloeistof","","Buitendiameter","mm","9.52","9.52","9.52"]
["","Gas","","Buitendiameter","mm","15.9","15.9","15.9"]
["","Drainage","","","mm","26x3","26x3","26x3"]
["","Hoogteverschil","","Max.","m","30","30","30"]
["Power supply","Phase","","","","3~","3~","3~"]
["","Frequentie","","","Hz","50","50","50"]
["","Naam","","","","Y1","Y1","Y1"]
["","Spanning","","","V","380-415","380-415","380-415"]
["Stroom","Afzekerwaarde","","","A","16","16","16"]
["Opmerkingen","","","","","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","(2) - Bevat gefluoreerde broeikasgassen","(2) - Bevat gefluoreerde broeikasgassen","(2) - Bevat gefluoreerde broeikasgassen"]