{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FCQG71FVEB / RZQSG71L3V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG100L9V1B","FCQG100FVEB / RZQSG100L9V1B","FCQG50FVEB / FCQG50FVEB / RZQSG100L9V1B","FCQG125FVEB / RZQSG125L9V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG125L9V1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQSG125L9V1B","FCQG60FVEB / FCQG60FVEB / RZQSG125L9V1B","FCQG140FVEB / RZQSG140L9V1B"]
["Totale koelcapaciteit","Nom.","","kW","6.8","","9.5","","12.0","","","","13.4"]
["Koeling","SEER","","","6.10","5.10","6.50","5.10","5.30","4.80","4.80","4.80"]
["","Jaarlijks energieverbruik","","kWu/a","390","652","512","652","793","875","875","875"]
["","Vermogen","Pdesign","kW","6.80","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Energieklasse","","","A++","B","A","B","A","B","B","B"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","6.33","7.60","7.60","7.60","8.03","7.60","7.60","7.60"]
["","SCOP/A","","","4.10","3.80","4.10","3.80","4.01","3.80","3.80","3.80"]
["","Energieklasse","","","A+","A","B","A","B","A","A","A"]
["","Jaarlijks energieverbruik","","kWu/a","2,162","2,800","2,596","2,800","2,804","2,800","2,800","2,800"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWu","1,060","","1,440","","1,870"]
["","EER","","","3.21","","3.30","","3.21","","","","3.01"]
["","COP","","","3.61","","3.54","","3.41","","","","3.41"]
["","Richtlijn Energielabels","Koeling","","A","","A","","A"]
["","","Verwarming","","A","","B","","B"]
["Totale verwarmingscapaciteit","Nom.","","kW","7.5","","10.8","","13.5","","","","15.5"]
["Opmerkingen","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]
["","","","","","","(3) - Jaarlijks energieverbruik is conform richtlijn 2002/31/EC inzake energielabels","","(3) - Jaarlijks energieverbruik is conform richtlijn 2002/31/EC inzake energielabels"]
["","","","","","","(4) - SEER en SCOP zijn conform EN 14825","","(4) - SEER en SCOP zijn conform EN 14825"]
["","","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]