{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A"]
[]
[]
[]
[]
["","","","","FHA35AVEB","FHA50AVEB","FHA60AVEB","FHA71AVEB"]
["Geluidsdrukniveau op 1 m","Verwarmen","Hoog","dB(A)","36","37","37","38"]
["","","Nom.","dB(A)","34","35","35","36"]
["","","Middelhoog","dB(A)","31","32","33","34"]
["","Koelen","Middelhoog","dB(A)","34","35","35","36"]
["","","Laag","dB(A)","31","32","33","34"]
["","","Hoog","dB(A)","36","37","37","38"]
["Standaard-accessoires","Thermische isolatiebuis","","","2","2","2","2"]
["","Draadklem","","","7","7","7","7"]
["","Slangband","","","1","1","1","1"]
["","Afvoerslang","","","1","1","1","1"]
["","Sluitring","","","8","8","8","8"]
["","Afdichtingskussen (groot)","","","1","1","1","1"]
["","Afdichtingskussen (klein)","","","1","1","1","1"]
["","Mof van kunsthars","","","1","1","1","1"]
["","Schroeven","","","2","2","2","2"]
["","Bedradingsklem","","","2","2","2","2"]
["Regelsystemen","Bedrade afstandsbediening","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7"]
["","Infrared remote control","","","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56"]
["Koelleidingmaten","Vloeistof","Buitendiameter","mm","6.35","6.35","6.35","9.52"]
["","Gas","Buitendiameter","mm","9.50","12.7","12.7","15.9"]
["","Afvoer","","","VP20","VP20","VP20","VP20"]
["Geluidsvermogenniveau","Koelen","","dB(A)","53","54","54","55"]
["Afmetingen","Unit","Breedte","mm","960","960","1,270","1,270"]
["","","Diepte","mm","690","690","690","690"]
["","","Hoogte","mm","235","235","235","235"]
["Behuizing","Materiaal","","","Kunsthars, metaalplaat","Kunsthars, metaalplaat","Kunsthars, metaalplaat","Kunsthars, metaalplaat"]
["","Kleur","","","Wit","Wit","Wit","Wit"]
["Gewicht","Unit","","kg","24.0","25.0","31.0","32.0"]
["Power supply","Fase","","","1~","1~","1~","1~"]
["","Frequentie","","Hz","50","50","50","50"]
["","Spanning","","V","220-240","220-240","220-240","220-240"]
["Opmerkingen","","","","(1) - Voor elektrische gegevens zie afzonderlijke tekening","(1) - Voor elektrische gegevens zie afzonderlijke tekening","(1) - Voor elektrische gegevens zie afzonderlijke tekening","(1) - Voor elektrische gegevens zie afzonderlijke tekening"]