{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Geluidsdrukniveau op 1 m","Verwarmen","Hoog","dB(A)","46"]
["","","Fluisterstille werking","dB(A)","30"]
["","","Laag","dB(A)","33"]
["","Koelen","Fluisterstille werking","dB(A)","29"]
["","","Laag","dB(A)","32"]
["","","Hoog","dB(A)","38"]
["","","Nom.","dB(A)","36"]
["","Koelen","Nom.","dB(A)","35"]
["Standaard-accessoires","Montagehandleiding","","","1"]
["","Bedieningshandleiding","","","1"]
["","Infrarood-afstandsbediening","","","1"]
["","AAA drogecelbatterij","","","2"]
["","Afstandsbedieningshouder","","","1"]
["","Montageplaat","","","1"]
["","Warmte-isolatiebuis (koelmiddelleidingen)","","","8"]
["","Luchtreinigingsfilter","","","1"]
["","Fotokatalytisch reukverdrijvend filter","","","1"]
["","Zijdeksel","","","2"]
["","Bundelband","","","4"]
["Regelsystemen","Infrared remote control","","","ARC433B67"]
["Leidingaansluitingen","Vloeistof","Buitendiameter","mm","6.35"]
["","Gas","Buitendiameter","mm","9.5"]
["","Afvoer","","","18"]
["Sound power level","Koelen","","dB(A)","53"]
["","Verwarmen","","dB(A)","59"]
["Afmetingen","Unit","Breedte","mm","1,050"]
["","","Diepte","mm","200"]
["","","Hoogte","mm","490"]
["Behuizing","Kleur","","","Amandelwit"]
["Gewicht","Unit","","kg","16"]
["Power supply","Fase","","","1~"]
["","Frequentie","","Hz","50"]
["","Naam","","","VM"]
["","Spanning","","V","220-240"]
["Opmerkingen","","","","(1) - 220V"]
["","","","","(2) - 230V"]
["","","","","(3) - 240V"]
["","","","","(4) - Wanneer aangesloten op een multisysteem buitenunit, raadpleeg dan de karakteristieken van de multibuitenunit die aangesloten moet worden."]