{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":7,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXL-JV"]
[]
[]
[]
[]
["","","","","","FTXL25J2V1B","FTXL35J2V1B"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.040, 0.040, 0.040","0.040, 0.040, 0.040"]
["","Verwarmen","","Nom.","kW","0.040, 0.040, 0.040","0.040, 0.040, 0.040"]
["Behuizing","Kleur","","","","Wit","Wit"]
["Afmetingen","Unit","","Hoogte","mm","283","283"]
["","","","Breedte","mm","770","770"]
["","","","Diepte","mm","198","198"]
["Gewicht","Unit","","","kg","8.00","8.00"]
["Ventilator-","Luchthoeveelheid","Koelen","Hoog","m³/min","9.3","9.3"]
["Ventilator","Luchtdebiet","Koeling","Middelhoog","m³/min","7.7","7.7"]
["Ventilator-","Luchthoeveelheid","Koelen","Laag","m³/min","6.1","6.1"]
["","","","Fluisterstille werking","m³/min","4.9","4.9"]
["","","Verwarmen","Hoog","m³/min","10.1","10.1"]
["Ventilator","Luchtdebiet","Verwarming","Middelhoog","m³/min","8.4","8.4"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Laag","m³/min","6.7","6.7"]
["","","","Fluisterstille werking","m³/min","5.7","5.7"]
["Geluidsvermogenniveau","Koelen","","","dBA","57","57"]
["","Verwarmen","","","dBA","57","57"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dBA","41","41"]
["Geluidsdrukniveau","Koeling","","Middelhoog","dBA","34","34"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dBA","27","27"]
["","","","Geluidsdrukniveau op 1 m-=-Koelen-=-Fluisterstille werking-=-dB(A)","dBA","23","23"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dBA","41","41"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dBA","35","35"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Laag-=-dB(A)","dBA","29","29"]
["","","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Fluisterstille werking-=-dB(A)","dBA","26","26"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35","6.35"]
["","Gas","","Buitendiameter","mm","9.50","9.50"]
["","Drainage","","","","18","18"]
["Regelsystemen","IR-afstandsbediening","","","","ARC433A87, ARC466A9","ARC433A87, ARC466A9"]
["Standaard-accessoires","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2"]
["","Batteries","","","","2","2"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Voeding","Naam","","","","V1","V1"]
["","Fase","","","","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","220-240","220-240"]
["Opmerkingen","","","","","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V"]