{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":9,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A"]
[]
[]
[]
[]
["","","","","","FVA71AMVEB","FVA100AMVEB","FVA125AMVEB","FVA140AMVEB"]
["Totale koelcapaciteit","Totale koelcapaciteit-=-Totale capaciteit","","Totale koelcapaciteit-=-Totale capaciteit-=-Nom.-=-kW","kW","","","12.10","13.40"]
["Verwarmingscapaciteit","Verwarmingscapaciteit-=-Totaalvermogen","","Verwarmingscapaciteit-=-Totaalvermogen-=-Nom.-=-kW","kW","","","13.5","15.5"]
["Behuizing","Behuizing-=-Kleur","","","","Zuiver wit","Zuiver wit","Zuiver wit","Zuiver wit"]
["Afmetingen","Afmetingen-=-Unit","","Afmetingen-=-Unit-=-Hoogte-=-mm","mm","1850","1850","1850","1850"]
["","","","Afmetingen-=-Unit-=-Breedte-=-mm","mm","600","600","600","600"]
["","","","Afmetingen-=-Unit-=-Diepte-=-mm","mm","270","350","350","350"]
["Gewicht","Gewicht-=-Unit-=-kg","","","kg","42","50","50","50"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Koelen","Ventilator--=-Luchthoeveelheid-=-Koelen-=-Hoog-=-m³/min","m³/min","18","28","28","30"]
["Ventilator","Ventilator-=-Luchtdebiet","Ventilator-=-Luchtdebiet-=-Koeling","Ventilator-=-Luchtdebiet-=-Koeling-=-Middelhoog-=-m³/min","m³/min","16","25","26","28"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Koelen","Ventilator--=-Luchthoeveelheid-=-Koelen-=-Laag-=-m³/min","m³/min","14","22","24","26"]
["","","Ventilator--=-Luchthoeveelheid-=-Verwarmen","Ventilator--=-Luchthoeveelheid-=-Verwarmen-=-Hoog-=-m³/min","m³/min","18","28","28","30"]
["Ventilator","Ventilator-=-Luchtdebiet","Ventilator-=-Luchtdebiet-=-Verwarming","Ventilator-=-Luchtdebiet-=-Verwarming-=-Middelhoog-=-m³/min","m³/min","16","25","26","28"]
["Ventilator-","Ventilator--=-Luchthoeveelheid","Ventilator--=-Luchthoeveelheid-=-Verwarmen","Ventilator--=-Luchthoeveelheid-=-Verwarmen-=-Laag-=-m³/min","m³/min","14","22","24","26"]
["Geluidsvermogenniveau","Geluidsvermogenniveau-=-Koelen-=-dBA","","","dB(A)","55","62","63","65"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dB(A)","43","50","51","53"]
["Geluidsdrukniveau","Geluidsdrukniveau-=-Koeling","","Geluidsdrukniveau-=-Koeling-=-Middelhoog-=-dBA","dB(A)","41","47","48","51"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dB(A)","38","44","46","48"]
["","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dB(A)","43","50","51","53"]
["Geluidsdrukniveau","Geluidsdrukniveau-=-Verwarming","","Geluidsdrukniveau-=-Verwarming-=-Middelhoog-=-dBA","dB(A)","38","44","46","48"]
["Geluidsdrukniveau op 1 m","Geluidsdrukniveau op 1 m-=-Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Nom.-=-dBA","dB(A)","41","47","48","51"]
["Leidingaansluitingen","Leidingaansluitingen-=-Vloeistof","","Leidingaansluitingen-=-Vloeistof-=-Buitendiameter-=-mm","mm","9.52","9.52","9.52","9.52"]
["","Leidingaansluitingen-=-Gas","","Leidingaansluitingen-=-Gas-=-Buitendiameter-=-mm","mm","15.9","15.9","15.9","15.9"]
["","Leidingaansluitingen-=-Drainage","","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Regelsystemen","Regelsystemen-=-Bedrade afstandsbediening","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standaard-accessoires","Installation manual","","","","1","1","1","1"]
["","Hole protection rubber","","","","2","2","2","2"]
["","Cover","","","","1","1","1","1"]
["","Dew proof material","","","","1","1","1","1"]
["","Remote control wiring","","","","1","1","1","1"]
["","Bracket for installation","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Bush","","","","1","1","1","1"]
["","Installation pattern","","","","1","1","1","1"]
["","Insulation for fitting for gas pipe","","","","1","1","1","1"]
["","Insulation for fitting for liquid pipe","","","","1","1","1","1"]
["","Screws","","","","5","5","5","5"]
["","Tie-wraps","","","","5","5","5","5"]
["Voeding","Voeding-=-Fase","","","","1~","1~","1~","1~"]
["Spanningsvorm","Spanningsvorm-=-Frequentie-=-Hz","","","Hz","50/60","50/60","50/60","50/60"]
["","Spanningsvorm-=-Spanning-=-V","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]