{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXS-F"]
[]
[]
[]
[]
["","","","","FVXS25FV1B (Archived)","FVXS35FV1B (Archived)","FVXS50FV1B (Archived)"]
["Geluidsdrukniveau op 1 m","Verwarmen","Hoog","dB(A)","38","39","45"]
["","","Fluisterstille werking","dB(A)","23","24","32"]
["","","Laag","dB(A)","26","27","36"]
["","Koelen","Fluisterstille werking","dB(A)","23","24","32"]
["","","Laag","dB(A)","26","27","36"]
["","","Hoog","dB(A)","38","39","44"]
["","","Nom.","dB(A)","32","33","40"]
["","Koelen","Nom.","dB(A)","32","33","40"]
["Standaard-accessoires","Montagehandleiding","","","1","1","1"]
["","Bedieningshandleiding","","","1","1","1"]
["","Draadloze afstandsbediening","","","1","1","1"]
["","Batterijen","","","2","2","2"]
["","Afstandsbedieningshouder","","","1","1","1"]
["","Afvoerslang","","","1","1","1"]
["","Luchttoevoer\nfilter","","","","1","1"]
["","Thermische isolatietape","","","2","2","2"]
["Besturingssystemen","Infrared remote control","","","ARC452A1","ARC452A1","ARC452A1"]
["Koelleidingmaten","Vloeistof","Buitendiameter","mm","6.35","6.35","6.35"]
["","Gas","Buitendiameter","mm","9.5","9.52","12.7"]
["","Afvoer","","","20","20","20"]
["Sound power level","Koelen","","dB(A)","52","52","60"]
["","Verwarmen","","dB(A)","52","52","60"]
["Afmetingen","Unit","Breedte","mm","700","700","700"]
["","","Diepte","mm","210","210","210"]
["","","Hoogte","mm","600","600","600"]
["Behuizing","Kleur","","","Wit","Wit","Wit"]
["Gewicht","Unit","","kg","14","14","14"]
["Power supply","Fase","","","1~","1~","1~"]
["","Frequentie","","Hz","50","50","50"]
["","Naam","","","V1","V1","V1"]
["","Spanning","","V","220-240","220-240","220-240"]
["Standaard-accessoires","Luchtreinigingsfilter","","","2"]
["Opmerkingen","","","","(1) - 220V","(1) - 220V"]
["","","","","(2) - 230V","(2) - 230V"]
["","","","","(3) - 240V","(3) - 240V"]
["","","","","(4) - Wanneer aangesloten op een multisysteem buitenunit, raadpleeg dan de karakteristieken van de multibuitenunit die aangesloten moet worden."]