{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":69,"n_cols":11,"rows_kept":69,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FWXT-ATV3CL"]
[]
[]
[]
[]
["","","","","","FWXT10AATV3CL","FWXT10ABTV3CL","FWXT15AATV3CL","FWXT15ABTV3CL","FWXT20AATV3CL","FWXT20ABTV3CL"]
["Koelvermogen","7/12°C","","Min.","kW","0.48","0.49","0.58","0.62","0.91","0.70"]
["","","","Med.","kW","0.80","0.88","1.03","1.08","1.75","1.21"]
["","","","Max.","kW","1.07","1.24","1.65","1.61","2.31","1.94"]
["Voelbaar koelvermogen","7/12°C","","Min.","kW","0.39","0.37","0.49","0.52","0.76","0.57"]
["","","","Med.","kW","0.69","0.70","0.91","0.86","1.53","1.02"]
["","","","Max.","kW","0.95","0.98","1.49","1.27","1.94","1.52"]
["Verwarmingscapaciteit","45/40°C","","Min.","kW","0.53","0.55","0.66","0.79","0.96","0.74"]
["","","","Med.","kW","0.94","1.00","1.26","1.36","1.98","1.55"]
["","","","Max.","kW","1.27","1.50","1.80","2.01","2.60","2.13"]
["Opgenomen vermogen","Min.","","","kW","0","0.01","0.01","0.01","0.01","0.01"]
["","Med.","","","kW","","0.01","","0.01","","0.01"]
["","Max.","","","kW","0.01","0.02","0.01","0.02","0.02","0.03"]
["Ventilatorsnelheid","Ventilatorsnelheid-=-Min.-=-rpm","","","rpm","84.00","680.00","124.00","680.00","138.00","680.00"]
["","Ventilatorsnelheid-=-Med.-=-rpm","","","rpm","155.00","1100.00","229.00","1100.00","283.00","1100.00"]
["","Ventilatorsnelheid-=-Max.-=-rpm","","","rpm","228.00","1500.00","331.00","1500.00","440.00","1500.00"]
["Behuizing","Kleur","","","","RAL 9003","RAL 9003","RAL 9003","RAL 9003","RAL 9003","RAL 9003"]
["","Materiaal","","","","Metaalplaat","Metaalplaat","Metaalplaat","Metaalplaat","Metaalplaat","Metaalplaat"]
["Afmetingen","Unit","","Hoogte","mm","335","335","335","335","335","335"]
["","","","Breedte","mm","902","902","1100","1102","1300","1302"]
["","","","Diepte","mm","128","128","128","128","128","128"]
["","Verpakte unit","","Hoogte","mm","490","490","490","490","490","490"]
["","","","Breedte","mm","1030","1030","1230","1230","1430","1430"]
["","","","Diepte","mm","210","210","210","210","210","210"]
["Gewicht","Unit","","","kg","14","14","16","16","19","19"]
["","Verpakte unit","","","kg","15","15","17","17","20","20"]
["Verpakking","Materiaal","","","","Karton","Karton","Karton","Karton","Karton","Karton"]
["","Gewicht","","","kg","1","1","1","1","1","1"]
["Warmtewisselaar","Aantal","","","","1","1","1","1","1","1"]
["","Volume interne spiraal","","","l","0.5","0.5","0.7","0.61","0.9","0.77"]
["","Vullen","","Bedrijfsdruk","bar","10","10","10","10","10","10"]
["Watercircuit","Diameter Koelleidingmaten","","","inch","3/4","3/4","3/4","3/4","3/4","3/4"]
["","Leidingsmateriaal","","","","Koper (CW617N)","KOPER","Koper (CW617N)","KOPER","Koper (CW617N)","KOPER"]
["","Druk","Verwarmen","Max.","bar","10","10","10","10","10","10"]
["Watercircuit - afname van de waterdruk","Verwarmen","45/40°C","Min.","kPa","1.10","5.10","2.80","4.81","1.10","6.00"]
["","","","Med.","kPa","3.10","12.00","3.50","6.30","4.10","6.40"]
["","","","Max.","kPa","5.40","16.30","4.00","7.20","6.60","8.10"]
["","Koelen","7/12°C","Min.","kPa","1.10","4.80","3.90","4.70","1.30","5.50"]
["","","","Med.","kPa","3.00","10.50","4.80","5.60","4.20","5.40"]
["","","","Max.","kPa","5.20","11.70","5.70","5.10","6.90","5.30"]
["Watercircuit - waterdebiet","Verwarmen","45/40°C","Min.","kg/u","91.90","100.00","112.60","140","164.80","150.00"]
["","","","Med.","kg/u","162.00","170.00","216.60","240","341.00","300.00"]
["","","","Max.","kg/u","218.40","260.00","310.00","350","447.20","420.00"]
["","Koelen","7/12°C","Min.","kg/u","82.10","80.00","98.90","110","156.50","120.00"]
["","","","Med.","kg/u","138.10","150.00","177.40","190","300.60","210.00"]
["","","","Max.","kg/u","184.40","210.00","283.00","280","396.80","330.00"]
["Geluidsniveau","Min.","","","dB(A)","34","35","34","36","35","37"]
["","Med.","","","dB(A)","","46","","47","","48"]
["","Geluidsniveau-=-Max.-=-dBA","","","dB(A)","49.0","53.0","51.0","54.0","52.0","55.0"]
["Werkingsbereik","Verwarmen","waterzijdig","Min.","°C","30","30","30","30","30","30"]
["","","","Max.","°C","85","85","85","85","85","85"]
["","Koelen","Waterzijde","Min.","°C","5","5","5","5","5","5"]
["","","","Max.","°C","18","18","18","18","18","18"]
["","Binnenopstelling","Omgeving","Min.","°C DB","0","0","0","0","0","0"]
["","","","Max.","°C DB","45","45","45","45","45","45"]
["Regelsystemen","IR-afstandsbediening","","","","","Voor FWXT-ATV3(C)(CL)","","Voor FWXT-ATV3(C)(CL)","","Voor FWXT-ATV3(C)(CL)"]
["","Geïntegreerd in binnenunit","","","","Nee","Ja","Nee","Ja","Nee","Ja"]
["Voeding","Fase","","","","1~","1~","1~","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50","50","50","50"]
["","Spanning","","","V","230","230","230","230","230","230"]
["Stroomverbruik","Max.","","","W","18","19","20","20","27","29"]
["","Stand-by","","","W","5","3","5","4","6","5"]
["Stroom","Max. bedrijfsstroom","","Verwarmen","A","0.2","0.16","0.2","0.18","0.2","0.24"]
["","","","Koelen","A","0.2","0.16","0.2","0.18","0.2","0.24"]