{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXDQ-M9"]
[]
[]
[]
[]
["","","","","FXDQ20M9V3B9","FXDQ25M9V3B9"]
["Koelmiddel","Type","","","R-410A","R-410A"]
["Koelleidingmaten","Vloeistof","Buitendiameter","mm","6.35","6.35"]
["","","Type","","Flareverbinding","Flareverbinding"]
["","Gas","Buitendiameter","mm","12.7","12.7"]
["","","Type","","Flareverbinding","Flareverbinding"]
["","Drainage","","","I.D. 21.6, O.D. 27.2","I.D. 21.6, O.D. 27.2"]
["Vereiste plafondruimte >","mm","","","250","250"]
["Afmetingen","Unit","Breedte","mm","502","502"]
["","","Diepte","mm","652","652"]
["","","Hoogte","mm","230","230"]
["Behuizing","Materiaal","","","Gegalvaniseerd staal","Gegalvaniseerd staal"]
["","Kleur","","","Ongelakt","Ongelakt"]
["Gewicht","Unit","","kg","17","17"]
["Power supply","Fase","","","1~","1~"]
["","Frequentie","","Hz","50","50"]
["","Naam","","","V1","V1"]
["","Spanning","","V","230","230"]
["Opmerkingen","","","","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 7,5m; hoogteverschil: 0m","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 7,5m; hoogteverschil: 0m"]
["","","","","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 7,5m; hoogteverschil: 0m","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 7,5m; hoogteverschil: 0m"]