{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":61,"n_cols":9,"rows_kept":61,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXUQ-A"]
[]
[]
[]
[]
["","","","","","FXUQ71AVEB","FXUQ71AVEB9","FXUQ100AVEB","FXUQ100AVEB9"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Bij hoge ventilatorsnelheid","dB(A)","40.0","40.0","47.0","47.0"]
["","","","Bij lage ventilatorsnelheid","dB(A)","36.0","36.0","40.0","40.0"]
["","","","Bij gemiddelde ventilatorsnelheid","dB(A)","38.0","38.0","44.0","44.0"]
["","Koelen","","Bij lage ventilatorsnelheid","dB(A)","36.0","36.0","40.0","40.0"]
["","","","Bij hoge ventilatorsnelheid","dB(A)","40.0","40.0","47.0","47.0"]
["","","","Bij gemiddelde ventilatorsnelheid","dB(A)","38.0","38.0","44.0","44.0"]
["Standaard-accessoires","Bedieningshandleiding","","","","Bedieningshandleiding","Bedieningshandleiding","Bedieningshandleiding","Bedieningshandleiding"]
["","Montagehandleiding","","","","Montagehandleiding","Montagehandleiding","Montagehandleiding","Montagehandleiding"]
["","Verklaring van conformiteit","","","","Verklaring van conformiteit","Verklaring van conformiteit","Verklaring van conformiteit","Verklaring van conformiteit"]
["","Afvoerslang","","","","Afvoerslang","Afvoerslang","Afvoerslang","Afvoerslang"]
["","Klemmetaal","","","","Klemmetaal","Klemmetaal","Klemmetaal","Klemmetaal"]
["","Sluitring voor ophangbeugel","","","","Sluitring voor ophangbeugel","Sluitring voor ophangbeugel","Sluitring voor ophangbeugel","Sluitring voor ophangbeugel"]
["","Klemmen","","","","Klemmen","Klemmen","Klemmen","Klemmen"]
["","Sluitklem","","","","Sluitklem","Sluitklem","Sluitklem","Sluitklem"]
["","Isolatiemateriaal koppelverbindingen","","","","Isolatiemateriaal koppelverbindingen","Isolatiemateriaal koppelverbindingen","Isolatiemateriaal koppelverbindingen","Isolatiemateriaal koppelverbindingen"]
["","Afdichtingsmateriaal","","","","Afdichtingsmateriaal","Afdichtingsmateriaal","Afdichtingsmateriaal","Afdichtingsmateriaal"]
["","Bochtstuk","","","","Bochtstuk","Bochtstuk","Bochtstuk","Bochtstuk"]
["","Montagepatroon","","","","Montagepatroon","Montagepatroon","Montagepatroon","Montagepatroon"]
["","Blokkeermateriaal","","","","Blokkeermateriaal","Blokkeermateriaal","Blokkeermateriaal","Blokkeermateriaal"]
["","L-vormige leiding","","","","L-vormige leiding","L-vormige leiding","L-vormige leiding","L-vormige leiding"]
["","Schroeven","","","","Schroeven","Schroeven","Schroeven","Schroeven"]
["","Non-woven textiel","","","","Non-woven textiel","Non-woven textiel","Non-woven textiel","Non-woven textiel"]
["Koudemiddel","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Type","","","","R-410A","R-410A","R-410A","R-410A"]
["Opgenomen vermogen","Koelen","","Bij hoge ventilatorsnelheid","kW","0.090","0.090","0.200","0.200"]
["","Verwarmen","","Bij hoge ventilatorsnelheid","kW","0.073","0.073","0.179","0.179"]
["Totale koelcapaciteit","Totaalvermogen","","Bij hoge ventilatorsnelheid","kW","8.0","8.0","11.2","11.2"]
["Koelleidingmaten","Vloeistof","","Buitendiameter","mm","9.52","9.5","9.52","9.5"]
["","","","Type","","Flareverbinding","Flareverbinding","Flareverbinding","Flareverbinding"]
["","Gas","","Buitendiameter","mm","15.9","15.9","15.9","15.9"]
["","","","Type","","Flareverbinding","Flareverbinding","Flareverbinding","Flareverbinding"]
["","Afvoer","","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Sound power level","Koelen","","Bij hoge ventilatorsnelheid","dB(A)","58","58","65","65"]
["Luchtfilter","Type","","","","Schimmelbestendig kunstharsnet","Schimmelbestendig kunstharsnet","Schimmelbestendig kunstharsnet","Schimmelbestendig kunstharsnet"]
["Afmetingen","Unit","","Breedte","mm","950","950","950","950"]
["","","","Diepte","mm","950","950","950","950"]
["","","","Hoogte","mm","198","198","198","198"]
["Behuizing","Materiaal","","","","Hars","Hars","Hars","Hars"]
["","Kleur","","","","Zuiver wit","Zuiver wit","Zuiver wit","Zuiver wit"]
["Gewicht","Unit","","","kg","26","26","27","27"]
["Ventilator","Luchthoeveelheid - 50Hz","Koelen","Bij hoge ventilatorsnelheid","m³/min","22.5","22.5","31.0","31.0"]
["","","","Bij lage ventilatorsnelheid","m³/min","16.0","16.0","21.0","21.0"]
["Totale verwarmingscapaciteit","Totaalvermogen","","Bij hoge ventilatorsnelheid","kW","9.0","9.0","12.5","12.5"]
["Stroom - 50Hz","Maximaal zekeringamperage (MFA)","","","A","16","16","16","16"]
["Power supply","Fase","","","","1~","1~","1~","1~"]
["","Frequentie","","","Hz","50/60","50/60","50/60","50/60"]
["","Spanning","","","V","220-240/220-230","220-240/220-230","220-240/220-230","220-240/220-230"]
["Opmerkingen","","","","","(1) - Spanningsbereik: de units zijn geschikt voor gebruik in elektrische systemen waar de spanning die over de aansluitklem van de unit wordt aangelegd binnen het opgegeven bereik ligt.","(1) - Spanningsbereik: de units zijn geschikt voor gebruik in elektrische systemen waar de spanning die over de aansluitklem van de unit wordt aangelegd binnen het opgegeven bereik ligt.","(1) - Spanningsbereik: de units zijn geschikt voor gebruik in elektrische systemen waar de spanning die over de aansluitklem van de unit wordt aangelegd binnen het opgegeven bereik ligt.","(1) - Spanningsbereik: de units zijn geschikt voor gebruik in elektrische systemen waar de spanning die over de aansluitklem van de unit wordt aangelegd binnen het opgegeven bereik ligt."]
["","","","","","(2) - De maximaal toegestane spanningsafwijking tussen de fasen bedraagt 2%.","(2) - De maximaal toegestane spanningsafwijking tussen de fasen bedraagt 2%.","(2) - De maximaal toegestane spanningsafwijking tussen de fasen bedraagt 2%.","(2) - De maximaal toegestane spanningsafwijking tussen de fasen bedraagt 2%."]
["","","","","","(3) - MCA / MFA : MCA = 1,25 x FLA","(3) - MCA / MFA : MCA = 1,25 x FLA","(3) - MCA / MFA : MCA = 1,25 x FLA","(3) - MCA / MFA : MCA = 1,25 x FLA"]
["","","","","","(4) - MFA ≤ 4 x FLA","(4) - MFA ≤ 4 x FLA","(4) - MFA ≤ 4 x FLA","(4) - MFA ≤ 4 x FLA"]
["","","","","","(5) - Volgende lagere standaardzekeringsterkte minimaal 16A","(5) - Volgende lagere standaardzekeringsterkte minimaal 16A","(5) - Volgende lagere standaardzekeringsterkte minimaal 16A","(5) - Volgende lagere standaardzekeringsterkte minimaal 16A"]
["","","","","","(6) - Kies een draaddikte op basis van de MCA-waarde","(6) - Kies een draaddikte op basis van de MCA-waarde","(6) - Kies een draaddikte op basis van de MCA-waarde","(6) - Kies een draaddikte op basis van de MCA-waarde"]
["","","","","","(7) - Gebruik een stroomonderbreker in plaats van een zekering","(7) - Gebruik een stroomonderbreker in plaats van een zekering","(7) - Gebruik een stroomonderbreker in plaats van een zekering","(7) - Gebruik een stroomonderbreker in plaats van een zekering"]
["","","","","","(8) - Bevat gefluoreerde broeikasgassen","(8) - Bevat gefluoreerde broeikasgassen","(8) - Bevat gefluoreerde broeikasgassen","(8) - Bevat gefluoreerde broeikasgassen"]