{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHCCU-CM3"]
[]
[]
[]
[]
["","","","","","JEHCCU0140CM3","JEHCCU0170CM3"]
["Koelvermogen","Matige temperatuur","R-407F","Nom","kW","2.08"]
["Gewicht","Unit","","","kg","67","68"]
["Opgenomen vermogen","Matige temperatuur","R-407F","Nom","kW","1.12"]
["COP","Medium temperature","","R-407F","","1.85"]
["Afmetingen","Unit","","Breedte","mm","1,101","1,101"]
["","","","Diepte","mm","444","444"]
["","","","Hoogte","mm","662","662"]
["Behuizing","Kleur","","","","Lichtgrijs","Lichtgrijs"]
["Ventilator","Type","","","","Axiaal","Axiaal"]
["Power supply","Fase","","","","3~","3~"]
["","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","400","400"]
["Opmerkingen","","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C"]
["","","","","","(2) - Geluidsdruk wordt gemeten op 10 m in anti-echo-kamer.","(2) - Geluidsdruk wordt gemeten op 10 m in anti-echo-kamer."]
["","","","","","(3) - Werkt op gefluoreerde broeikasgassen","(3) - Werkt op gefluoreerde broeikasgassen"]