{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":136,"n_cols":14,"rows_kept":136,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHSCU-CL3"]
[]
[]
[]
[]
["","","","","","JEHSCU0300CL3","JEHSCU0400CL3","JEHSCU0500CL3","JEHSCU0600CL3","JEHSCU0750CL3","JEHSCU0951CL3 EVI","JEHSCU0951CL3 EVI_","JEHSCU0200CL3 (Archived)","JEHSCU0950CL3 EVI (Archived)"]
["Koelvermogen","Lage temperatuur","R-407F","Nom","kW","","2.38","2.87","","","","","","4.88"]
["Jaarlijks elektriciteitsverbruik Q","R-407F","","Te -35°C","kWu/a","","10,730.00","13,018.00","","","","","","22,348.00"]
["Parameters bij vollast en omgevingstemp. 43°C","R-407F","Te -35°C","Opgenomen vermogen (D3)","kW","","3.30"]
["","","","Cooling capacity (P3)","kW","","2.04"]
["","","","Vermelde COP (COP3)","","","0.62"]
["Gewicht","Unit","","","kg","78","132","132","133","203","","","76","200"]
["Koudemiddel","GWP","","","","","","","","","","","3,922"]
["","Type","","","","","","","","","","","R-404A"]
["SEPR (seizoensgebaseerde energieprestatie-ratio)","R-407F","","Te -35°C","","","1.65","1.64","","","","","","1.63"]
["Parameters bij vollast en omgevingstemp. 32°C (punt A)","R-407F","Te -35°C","Nom. opgenomen vermogen (DA)","kW","","2.51","3.08","","","","","","4.51"]
["","","","Nom. COP (COPA)","","","0.95","0.93","","","","","","1.08"]
["","","","Nom. koelvermogen (PA)","kW","","2.38","2.87","","","","","","4.88"]
["COP","Low temperature","","R-407F","","","0.95","0.93","","","","","","1.08"]
["Afmetingen","Unit","","Breedte","mm","1,101","1,353","1,353","1,353","1,348","","","1,101","1,348"]
["","","","Diepte","mm","444","575","575","575","605","","","444","605"]
["","","","Hoogte","mm","662","872","872","872","1,727","","","662","1,727"]
["Behuizing","Kleur","","","","Lichtgrijs","Lichtgrijs","Lichtgrijs","Lichtgrijs","Lichtgrijs","","","Lichtgrijs","Lichtgrijs"]
["Ventilator","Type","","","","Axiaal","Axiaal","Axiaal","Axiaal","Axiaal","","","Axiaal","Axiaal"]
["Power supply","Fase","","","","3~","3~","3~","3~","3~","","","3~","3~"]
["","Frequentie","","","Hz","50","50","50","50","50","","","50","50"]
["","Spanning","","","V","400","400","400","400","400","","","400","400"]
["Opmerkingen","","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - Raadpleeg de condities: Buitentemperatuur = 32°C, verdampingstemperatuur = -10°C en 10K superverwarming (toepassing met matige temperatuur)"]
["","","","","","(2) - Geluidsdruk wordt gemeten op 10 m in anti-echo-kamer.","(2) - Geluidsdruk wordt gemeten op 10 m in anti-echo-kamer.","(2) - Geluidsdruk wordt gemeten op 10 m in anti-echo-kamer.","(2) - Geluidsdruk wordt gemeten op 10 m in anti-echo-kamer.","(2) - Geluidsdruk wordt gemeten op 10 m in anti-echo-kamer.","","","(2) - Geluidsdruk wordt gemeten op 10 m in anti-echo-kamer.","(2) - Geluidsdruk wordt gemeten op 10 m in anti-echo-kamer."]
["","","","","","(3) - Werkt op gefluoreerde broeikasgassen","(3) - Werkt op gefluoreerde broeikasgassen","(3) - Werkt op gefluoreerde broeikasgassen","(3) - Werkt op gefluoreerde broeikasgassen","(3) - Werkt op gefluoreerde broeikasgassen","","","(3) - Werkt op gefluoreerde broeikasgassen","(3) - Werkt op gefluoreerde broeikasgassen"]
["Koelvermogen","Lage temperatuur","R-448A","Nom.","kW","1.62","2.53","","3.49","4.81"]
["","","R-449A","Nom.","kW","1.62","2.53","","3.49","4.81"]
["Parameters bij vollast en omgevingstemp. 43°C","R-449A","Te -35°C","Vermelde COP (COP3)","","0.68","0.68","","0.46","0.81"]
["","","","Opgenomen vermogen (D3)","kW","2.11","3.29","","6.15","5.28"]
["","","","Koelvermogen (P3)","kW","1.43","2.23","","2.82","4.26"]
["","R-448A","Te -35°C","Opgenomen vermogen (D3)","kW","2.11","3.29","","6.15","5.28"]
["","","","Vermelde COP (COP3)","","0.68","0.68","","0.46","0.81"]
["","","","Koelvermogen (P3)","kW","1.43","2.23","","2.82","4.26"]
["Parameters bij vollast en omgevingstemp. 25°C","R-449A","Te -35°C","Vermelde COP (COP2)","","1.16"]
["","","","Opgenomen vermogen (D2)","kW","1.48"]
["","","","Koelvermogen (P2)","kW","1.71"]
["","R-448A","Te -35°C","Koelvermogen (P2)","kW","1.71"]
["","","","Opgenomen vermogen (D2)","kW","1.48"]
["","","","Vermelde COP (COP2)","","1.16"]
["Koudemiddel","GWP type 5","","","","1,387","1,387","","1,387","1,387"]
["","Type 5","","","","R-448A","R-448A","","R-448A","R-448A"]
["Parameters bij vollast en omgevingstemp. 32°C (punt A)","R-448A","Te -35°C","Nom. opgenomen vermogen (DA)","kW","1.67","2.48","","4.19","4.08"]
["","","","Nom. COP (COPA)","","0.97","1.02","","0.83","1.18"]
["","","","Nom. koelvermogen (PA)","kW","1.62","2.53","","3.49","4.81"]
["","R-449A","Te -35°C","Nom. koelvermogen (PA)","kW","1.62","2.53","","3.49","4.81"]
["","","","Nom. COP (COPA)","","0.97","1.02","","0.83","1.18"]
["","","","Nom. opgenomen vermogen (DA)","kW","1.67","2.48","","4.19","4.08"]
["Opgenomen vermogen","Lage temperatuur","R-448A","Nom.","kW","1.67","2.48","","4.19","4.08"]
["","","R-449A","Nom.","kW","1.67","2.48","","4.19","4.08"]
["COP","Low temperature","","R-449A","","0.97","1.02","","0.83","1.18"]
["","","","R-448A","","0.97","1.02","","0.83","1.18"]
["Koelvermogen","Lage temperatuur","R-407A","Nom","kW","","2.29","2.77","3.31"]
["Jaarlijks elektriciteitsverbruik Q","R-407A","","Te -35°C","kWu/a","","10,212.00","12,364.00","15,026.00"]
["","R-449A","","Te -35°C","kWu/a","","11,276.00","","15,878.00","21,856.00"]
["","R-448A","","Te -35°C","kWu/a","","11,276.00","","15,878.00","21,856.00"]
["Parameters bij vollast en omgevingstemp. 43°C","R-407A","Te -35°C","Koelvermogen (P3)","kW","","2.01","2.40","2.88"]
["","","","Vermelde COP (COP3)","","","0.67","0.66","0.64"]
["","","","Opgenomen vermogen (D3)","kW","","2.98","3.64","4.48"]
["SEPR (seizoensgebaseerde energieprestatie-ratio)","R-448A","","Te -35°C","","","1.67","","1.64","1.64"]
["","R-449A","","Te -35°C","","","1.67","","1.64","1.64"]
["","R-407A","","Te -35°C","","","1.67","1.67","1.64"]
["Koudemiddel","GWP type 2","","","","","2,107","2,107","2,107"]
["","GWP type 3","","","","","1,825","1,825"]
["","Type 3","","","","","R-407F","R-407F"]
["","Type 2","","","","","R-407A","R-407A","R-407A"]
["Parameters bij vollast en omgevingstemp. 32°C (punt A)","R-407A","Te -35°C","Nom. COP (COPA)","","","0.98","0.97","0.93"]
["","","","Nom. koelvermogen (PA)","kW","","2.29","2.77","3.31"]
["","","","Nom. opgenomen vermogen (DA)","kW","","2.33","2.85","3.57"]
["Opgenomen vermogen","Lage temperatuur","R-407A","Nom","kW","","2.33","2.85","3.57"]
["COP","Low temperature","","R-407A","","","0.98","0.97","0.93"]
["Koelvermogen","Lage temperatuur","R-407A","Nom","kW","","","","","","4.89","4.89"]
["","","R-407F","Nom","kW","","","","","","4.90","4.90"]
["Koelcapaciteit","Lage temperatuur","R-448A","Nom.","kW","","","","","","4.85","4.85"]
["","","R-449A","Nom.","kW","","","","","","4.85","4.85"]
["Opgenomen vermogen","Lage temperatuur","R-407A","Nom","kW","","","","","","4.15","4.15"]
["","","R-407F","Nom","kW","","","","","","3.86","3.86"]
["","","R-448A","Nom.","kW","","","","","","3.95","3.95"]
["","","R-449A","Nom.","kW","","","","","","3.95","3.95"]
["Prestatiecoëfficiënt (COP)","Lage temperatuur","","R-407A","","","","","","","1.18","1.18"]
["COP","Lage temperatuur","","R-407F","","","","","","","1.27","1.27"]
["Prestatiecoëfficiënt (COP)","Lage temperatuur","","R-448A","","","","","","","1.23","1.23"]
["","","","R-449A","","","","","","","1.23","1.23"]
["Jaarlijks elektriciteitsverbruik Q","R-407A","","Te -35°C","kWu/a","","","","","","22108.00","22108.00"]
["","R-407F","","Te -35°C","kWu/a","","","","","","20961.00","20961.00"]
["","R-448A","","Te -35°C","kWu/a","","","","","","21477.00","21477.00"]
["","R-449A","","Te -35°C","kWu/a","","","","","","21477.00","21477.00"]
["SEPR (seizoensgebaseerde energieprestatie-ratio)","R-407A","","Te -35°C","","","","","","","1.65","1.65"]
["","R-407F","","Te -35°C","","","","","","","1.74","1.74"]
["","R-448A","","Te -35°C","","","","","","","1.68","1.68"]
["","R-449A","","Te -35°C","","","","","","","1.68","1.68"]
["Parameters bij vollast en omgevingstemp. 32°C (punt A)","R-407A","Te -35°C","Nom. koelvermogen (PA)","kW","","","","","","4.89","4.89"]
["","","","Nom. opgenomen vermogen (DA)","kW","","","","","","3.15","3.15"]
["","","","Nom. COP (COPA)","","","","","","","1.18","1.18"]
["","R-407F","Te -35°C","Nom. koelvermogen (PA)","kW","","","","","","4.90","4.90"]
["","","","Nom. opgenomen vermogen (DA)","kW","","","","","","3.86","3.86"]
["","","","Nom. COP (COPA)","","","","","","","1.27","1.27"]
["","R-448A","Te -35°C","Nom. koelvermogen (PA)","kW","","","","","","4.85","4.85"]
["","","","Nom. opgenomen vermogen (DA)","kW","","","","","","3.95","3.95"]
["","","","Nom. COP (COPA)","","","","","","","1.23","1.23"]
["","R-449A","Te -35°C","Nom. koelvermogen (PA)","kW","","","","","","4.85","4.85"]
["","","","Nom. opgenomen vermogen (DA)","kW","","","","","","3.95","3.95"]
["","","","Nom. COP (COPA)","","","","","","","1.23","1.23"]
["Behuizing","Kleur","","","","","","","","","Lichtgrijs","Lichtgrijs"]
["Afmetingen","Unit","","Hoogte","mm","","","","","","1727","1727"]
["","","","Breedte","mm","","","","","","1348","1348"]
["","","","Diepte","mm","","","","","","605","605"]
["Gewicht","Unit","","","kg","","","","","","200","200"]
["Ventilator","Type","","","","","","","","","Axiaal","Axiaal"]
["Koelmiddel","Type 2","","","","","","","","","R-407A","R-407A"]
["","Type 3","","","","","","","","","R-407F","R-407F"]
["","Type 5","","","","","","","","","R-448A","R-448A"]
["","GWP type 2","","","","","","","","","2107","2107"]
["","Koelmiddel-=-GWP type 3","","","","","","","","","1825","1825"]
["","GWP type 5","","","","","","","","","1387","1387"]
["Voeding","Fase","","","","","","","","","3~","3~"]
["Spanningsvorm","Frequentie","","","Hz","","","","","","50","50"]
["","Spanning","","","V","","","","","","400","400"]
["Unit","Nominale bedrijfsspanning (RLA)","R-448A","Koelen","A","","","","","","8.50","8.50"]
["","","R-449A","Koelen","A","","","","","","8.50","8.50"]
["Opmerkingen","","","","","","","","","","(2) - Geluidsdruk wordt gemeten op 10 m in anti-echo-kamer.","(2) - Geluidsdruk wordt gemeten op 10 m in anti-echo-kamer."]
["Jaarlijks elektriciteitsverbruik Q","R-404A","","Te -35°C","kWu/a","","","","","","","24503"]
["SEPR (seizoensgebaseerde energieprestatie-ratio)","R-404A","","Te -35°C","","","","","","","","1.79"]
["Parameters bij vollast en omgevingstemp. 32°C (punt A)","R-404A","Te -35°C","Nom. koelvermogen (PA)","kW","","","","","","","5.90"]
["","","","Nom. opgenomen vermogen (DA)","kW","","","","","","","4.35"]
["","","","Nom. COP (COPA)","","","","","","","","1.36"]
["Parameters bij vollast en omgevingstemp. 43°C","R-404A","Te -35°C","Vermelde COP (COP3)","","","","","","","","1.06"]
["Parameters bij vollast en omgevingstemp. 32°C (punt A)","R-404A","Te -35°C","Nom. koelvermogen (PA)","kW","","","","","","","","1.42"]
["","","","Nom. opgenomen vermogen (DA)","kW","","","","","","","","1.46"]
["","","","Nom. COP (COPA)","","","","","","","","","0.97"]
["Parameters bij vollast en omgevingstemp. 25°C","R-404A","Te -35°C","Vermelde COP (COP2)","","","","","","","","","1.16"]
["Parameters bij vollast en omgevingstemp. 43°C","R-404A","Te -35°C","Vermelde COP (COP3)","","","","","","","","","0.60"]