{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHSCU-CM1"]
[]
[]
[]
[]
["","","","","","JEHSCU0200CM1","JEHSCU0250CM1","JEHSCU0300CM1"]
["Koelcapaciteit","Middelhoge temperatuur","R-134a","Nom","kW","2.13"]
["","","R-407F","Nom","kW","3.33","3.82","4.63"]
["Parameters bij vollast en omgevingstemp. 43°C","R-134a","Te -10°C","Power input (D3)","kW","1.32"]
["","","","Vermelde COP (COP3)","","1.42"]
["","","","Koelvermogen (P3)","kW","1.87"]
["Gewicht","Unit","","","kg","69.7","71.7","73.7"]
["Koelmiddel","GWP","","","","1,430"]
["","Type","","","","R-134a"]
["Parameters bij vollast en omgevingstemp. 32°C (punt A)","R-134a","Te -10°C","Nom. COP (COPA)","","1.92"]
["","","","Nom. koelvermogen (PA)","kW","2.13"]
["","","","Nom. opgenomen vermogen (DA)","kW","1.11"]
["Opgenomen vermogen","Matige temperatuur","R-407F","Nom","kW","1.74","2.09","2.66"]
["","","R-134a","Nom","kW","1.11"]
["COP","Medium temperature","","R-134a","","1.92"]
["","","","R-407F","","1.92","1.83","1.74"]
["Afmetingen","Unit","","Breedte","mm","1,101","1,101","1,101"]
["","","","Diepte","mm","444","444","444"]
["","","","Hoogte","mm","662","662","662"]
["Behuizing","Kleur","","","","Lichtgrijs","Lichtgrijs","Lichtgrijs"]
["Ventilator","Type","","","","Axiaal","Axiaal","Axiaal"]
["Power supply","Fase","","","","1~","1~","1~"]
["","Frequentie","","","Hz","50","50","50"]
["","Spanning","","","V","230","230","230"]
["Opmerkingen","","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C"]
["","","","","","(2) - Geluidsdruk wordt gemeten op 10 m in anti-echo-kamer.","(2) - Geluidsdruk wordt gemeten op 10 m in anti-echo-kamer.","(2) - Geluidsdruk wordt gemeten op 10 m in anti-echo-kamer."]
["","","","","","(3) - Werkt op gefluoreerde broeikasgassen","(3) - Werkt op gefluoreerde broeikasgassen","(3) - Werkt op gefluoreerde broeikasgassen"]