{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":9,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXN-MB"]
[]
[]
[]
[]
["","","","","","RXN60MV1B","RXN25MV1B (Archived)","RXN35MV1B (Archived)","RXN50MV1B (Archived)"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Nom.","dB(A)","51"]
["","Koelen","","Nom.","dB(A)","51"]
["Koelmiddel","Charge","","","TCO2Eq","3"]
["","GWP","","","","2,087.5"]
["","Vulling","","","kg","1.45"]
["","Type","","","","R-410A"]
["Compressor","Type","","","","Hermetische swing"]
["Afmetingen","Unit","","Breedte","mm","855"]
["","","","Diepte","mm","328"]
["","","","Hoogte","mm","753"]
["Gewicht","Unit","","","kg","44"]
["Power supply","Fase","","","","1~"]
["","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-240"]
["Opmerkingen","","","","","(1) - Alle specificaties kunnen door de fabrikant worden gewijzigd zonder voorafgaande mededeling."]
["","","","","","(2) - Bevat gefluoreerde broeikasgassen"]
["Afmetingen","Unit","","Hoogte","mm","","550","550","753"]
["","","","Breedte","mm","","658","658","855"]
["","","","Diepte","mm","","289","289","328"]
["Gewicht","Unit","","","kg","","31","31","44"]
["Compressor","Type","","","","","Hermetische swing","Hermetische swing","Hermetische swing"]
["Werkingsbereik","Koelen","","Min.","°CDB","","10","10","-10"]
["","","","Max.","°CDB","","46","46","46"]
["","Verwarmen","","Min.","°CWB","","-15","-15","-15"]
["","","","Max.","°CWB","","18","18","18"]
["Geluidsdrukniveau op 1 m","Koelen","","Nom.","dB(A)","","45","46","51"]
["","Verwarmen","","Nom.","dB(A)","","45","46","51"]
["Koelmiddel","Type","","","","","R-410A","R-410A","R-410A"]
["","Vulling","","","kg","","1.00","1.00","1.45"]
["Koudemiddel","Vulling","","","tCO2Eq","","2.1","2.1","3"]
["Koelmiddel","GWP","","","","","2087.5","2087.5","2087.5"]
["Koelleidingmaten","Leidinglengte","","Max.","m","","20","20","30"]
["Voeding","Fase","","","","","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","","50","50","50"]
["","Spanning","","","V","","220-240","220-240","220-240"]