{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Afmetingen","Unit","","Hoogte","mm","870","870"]
["","","","Breedte","mm","1,100","1,100"]
["","","","Diepte","mm","460","460"]
["Gewicht","Unit","","","kg","117","117"]
["Compressor","Type","","","","Hermetisch gesloten scrollcompressor","Hermetisch gesloten scrollcompressor"]
["Werkingsbereik","Koelen","","Min.","°CDB","-20","-20"]
["","","","Max.","°CDB","46","46"]
["","Verwarmen","Max.","Min.","°CWB","-20","-20"]
["","","","Max.","°CWB","15","15"]
["Sound power level","Koelen","","","dB(A)","73","76"]
["","Verwarmen","","","dB(A)","76 (1)","79 (1)"]
["Geluidsdrukniveau op 1 m","Koelen","","Nom.","dB(A)","53","57"]
["","Verwarmen","","Nom.","dB(A)","60","63"]
["Koelmiddel","Type","","","","R-32","R-32"]
["","Charge","","","kg","5","5"]
["","GWP","","","","675","675"]
["Koelleidingmaten","Vloeistof","","Buitendiameter","mm","9.52","9.52"]
["","Gas","","Buitendiameter","mm","22.2","22.2"]
["","Leidinglengte","","Max.","m","100","100"]
["","","Voorgevuld tot","","m","30","30"]
["","Bijkomende koelmiddelvulling","","","kg/m","Zie installatiehandleiding","Zie installatiehandleiding"]
["Standaard-accessoires","Montagehandleiding","","","","1","1"]
["","Algemene voorzorgsmaatregelen","","","","1","1"]
["","Kabelbinders","","","","2","2"]
["","Stickervel met F-gaslabel","","","","1","1"]
["","Aansluitleidingen","","","","6","6"]
["Power supply","Fase","","","","3~","3~"]
["","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","380-415","380-415"]
["Stroom - 50Hz","Maximaal zekeringamperage (MFA)","","","A","20","20"]
["Opmerkingen","","","","","(1) - Volgens ENER Lot 21","(1) - Volgens ENER Lot 21"]