{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":9,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RZAG-B"]
[]
[]
[]
[]
["","","","","FDXM35F3V1B9 / RZAG35B5V1B","FDXM50F3V1B9 / RZAG35B5V1B","FDXM50F3V1B9 / RZAG50B5V1B","FDXM60F3V1B9 / RZAG50B5V1B","FDXM60F3V1B9 / RZAG60B5V1B"]
["Totale koelcapaciteit","Min.","","kW","1.6","1.6","1.7","1.7","1.7"]
["","Nom.","","kW","3.5","3.5","5","5","6"]
["","Max.","","kW","4.5","4.5","6","6","6.5"]
["Totale verwarmingscapaciteit","Min.","","kW","1.4","1.4","1.7","1.7","1.7"]
["","Nom.","","kW","4","4","5","5","7"]
["","Max.","","kW","5","5","6","6","7.5"]
["Nominaal rendement","EER","","","3.9","4.05","3.8","3.98","3.4"]
["","COP","","","3.5","3.63","3.4","3.44","3.3"]
["","Jaarlijks energieverbruik","","kWu","449","432","658","628","882"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","A","A","A","A","A"]
["","","Verwarming","","B","A","C","B","C"]
["Koeling","Koeling-=-Energieklasse","","","A+","A+","A+","A+","A+"]
["","Vermogen","Pdesign","kW","3.5","3.5","5","5","6"]
["","SEER","","","5.9","6.08","5.9","5.98","5.7"]
["","Jaarlijks energieverbruik","","kWu/a","208","201","296","293","368"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A","A+","A","A","A"]
["","Vermogen","Pdesign","kW","3.5","4.2","4.3","4.3","4.5"]
["","SCOP/A","","","3.9","4.05","3.9","3.94","3.9"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","2.99","3.49","3.62","3.63","3.82"]
["","Jaarlijks energieverbruik","","kWu/a","1255","1451","1544","1526","1616"]