{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC073"]
[]
[]
[]
[]
["","","","","BRC073A1"]
["Verpakking","Materiaal","","","Karton_"]
["","Gewicht","","kg","0.050"]
["Omgevingstemperatuur","Relatieve vochtigheid <","","%","95"]
["","Bewaring","Min.","°C","-20"]
["","","Max.","°C","70"]
["","Bedrijf","Min.","°C","-10"]
["","","Max.","°C","50"]
["Temperatuurinstelling","Resolutie","","°C","1"]
["","Bereik instelpunt","Koelen","°C","18-32"]
["","","Verwarmen","°C","10-30"]
["Afmetingen","Verpakte unit","Breedte","mm","220"]
["","","Hoogte","mm","50"]
["","","Diepte","mm","160"]
["","Unit","Breedte","mm","120"]
["","","Diepte","mm","19"]
["","","Hoogte","mm","120"]
["Behuizing","Deksel knop","","","Nee"]
["","Colour","","","Zuiver wit"]
["","Bedrijfs LED","Kleur","","Groen"]
["LCD","Type","","","Full dot (160 x 255)"]
["","Achtergrondverlichting","Kleur","","Wit"]
["","Afmetingen","B","mm","68.85"]
["","","H","mm","43.2"]
["Gewicht","Verpakte unit","","kg","0.348"]
["","Unit","","kg","0.290"]